SUPLEMENTARY MATERIAL TO

**The synthesis of transparent TiO2 photoelectrodes assisted by rheological agent (Triton X-100, PVP and F-127) for dye sensitized solar cells.**

Joan Reyes Miranda1, Ángel de Jesús Morales Ramírez1[[1]](#footnote-1)\* Felipe de Jesús Carrillo Romo1, Antonieta García Murillo1, Elder de la Rosa Cruz2, César A. Flores Sandoval3, Aristeo Garrido Hernández4, and Dulce Yolotzin Medina Velázquez5

C:\Users\Joan\AppData\Local\Microsoft\Windows\INetCache\Content.Word\Fig. 2.tif

Fig. S-1**.** Infrared spectra of the TiO2 powders in the presence of Triton (a), PVP (b) and F-127 (c) at 500° C for 60 minutes.

C:\Users\Joan\AppData\Local\Microsoft\Windows\INetCache\Content.Word\Fig. 6.tif

Fig.S-2**.** (αhυ)0.5 versus photon energy (hυ) for indirect band gap of Triton and PVP assisted TiO2 films.

C:\Users\Joan\AppData\Local\Microsoft\Windows\INetCache\Content.Word\Fig. 7.tif

Fig. S-3**.** Evolution of the density and porosity of the TiO2 films as a function of the molar ratios of the RAs: (a) Triton, (b) PVP, (c) F-127.

C:\Users\Joan\AppData\Local\Microsoft\Windows\INetCache\Content.Word\Fig. S-4.tif

Fig. S-4. Band energy diagram indicating the energy levels and the process that describe the electron injection from the dye to the conduction band of TiO2

1. \*Corresponding author. E-mail: angel\_ipn77@hotmail.com [↑](#footnote-ref-1)